1 Extract the zip files to a temporary directory
2 Run set up
3 Run lanlink by clicking on the lanlink.exe file in the lanlink directory
4 Ignore any error messages
5 Click on the Tools menu item on the top line
6 Click on the settings option
7 Go through each notebook page and change the appropriate parameters
8 Save the settings using the button below the notebook page
9 Click on the File menu item on the top line
10 Edit the ini files to change the calls to your call
11 In the lanlink.ini files, change the com port to that you wish to use for your
    tnc interface. If you are not using a tnc, then set it to 0.
12 Set the appropriate default mode. Change it to psk31 if you are only using 
    the sound card interface.
13 Save the lanlink.ini file and exit from the editor.
14 Exit lanlink  do not save or load the settings before you exit.
15 Restart lanlink and all should be well
