Variable    Value            Meaning
--------    -----            -------
<IGATE>     No\Yes          Is IGate open and available
<IGATE2>    Down\Up         Is IGate open and available
<FILLER>    No\Yes          Is Channel Filler on
<INET>      Unknown\No\Yes  Is an Internet Connection Available  (Win95/98 = Yes/No)  WinNT=Unknown
<VER>       ###XX           Version of APRS+SA
<TTS>       No\Yes          Is Text-To-Speak Enabled
<SA>        SAx             Version of Street Atlas being used
<TNC>       Name.tnc        TNC file in use
<UP>        Days:hr:min:sec Time since program was last restarted
<WWW>       No\Yes          Is Web Server enabled
<URL>       Web Address     URL of APRS+SA Web server if enabled
<UNIQUE>    9999            Number of Unique stations with Position
<POSITS>    9999            Current number of unique position reports
<TAC>       Tac Call        Tactical Callsign
<LOC>	    Location	    Location as entered on Profile page of setup
<EMAIL>     Email Address   Email address as entered on the Profile page of Setup
<NAME>      Name            Name as entered on Profile page of Setup
<HOMEPAGE>  Web Address     Web Address as entered on Profile page of Setup
<TS>        Date/Time       Date/Time packet was received the first time
<WSTS>      Date/Time       Workspace Date/Time.  When program was compiled.
<GS4>       Grid Square     Grid Square - 4  character
<GS6>       Grid Square     Grid Square - 6  character
<GS8>       Grid Square     Grid Square - 8  character
<GS10>      Grid Square     Grid Square - 10 character
<GS12>      Grid Square     Grid Square - 12 character
<GS14>      Grid Square     Grid Square - 14 character

